**Edgewood Avenue**

**Public Right-of-Way Construction Impacts**

**Side:** North

**Limits:** Ladson to Marvin

**Sidewalk Width:** 5-Ft

**Sidewalk Material:** Concrete

**Road Width:** 32’ (gutter to gutter)

|  |  |
| --- | --- |
| **ADDRESS** | **CONSTRUCTION IMPACTS** |
| **For All Addresses** | Construct a 5’ wide concrete sidewalk with a 2-3’ green space.Remove a total of 200 LF of curb and replace with barrier curb. |
| **318 Ladson**  | Place sidewalk behind fire hydrant. Construct a retaining wall or backer curb as needed to tie into existing grade.Remove and replace concrete driveway apron. Place sidewalk behind utility pole. |
| **315 Marvin** | Place sidewalk behind traffic sign and support. Remove bush.Remove and replace concrete driveway apron. Place sidewalk behind storm drain inlet structure. |

**☞ The above impacts are based on a preliminary investigation and are subject to change at any time as field conditions warrant.**